

**IMPORTANT INFORMATION**

**PCB v1.2**

1. Transistor Q1 should be reversed. Mount with the flat side of the transistor facing the bottom of the PCB.

A close up of a circuit board

Description automatically generated

1. Capacitors C3 and C4 are marked 103. The supplied 100nF (104) capacitors should be used here.

A close up of a circuit board

Description automatically generated

For latest information, firmware, software, tutorials, check out:

**GitHub:** [**https://github.com/visrealm/pico-56**](https://github.com/visrealm/pico-56)

**YouTube: https://youtube.com/@TroySchrapel**